

**ELECTRIC CONVECTION PATISSERIE OVEN**

**PATISSERIE OVENS**





The stainless steel body makes the device durable and enduring.

Easy to clean through its rounded internal chamber corners.

Its openable internal glass ensures easy cleaning.

It is composed with high temperature resistant double glazing.

The insulation material around the cabinet minimizes heat loss and saves energy.

The special door seal prevents heat transition from the door and saves energy.

Double direction rotatable stainless steel fan ensures homogeneous heat distribution in the cabinet.

The safety thermostat prevents overheating of the cabinet.

Offers manual or automatic humidity control.

All functions are digitally controlled.

Offers a wide cooking range with its up to 180 minutes adjustable cooking time.

Prepares the oven for the next cooking with its cooling function.

99 programmable cooking memories with 4 adjustable cooking stages.

Safety door switch stops the cooking process in case the door opens.

Halogen lamps are used for the internal lightening.

With a capacity of 4 x 40x60 mm or 4 x GN 1/1 40 mm trays.



EI=ELECTRIC INLET

WI=WATER INLET

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **MODEL** | **DESCRIPTION** | **DIMENSIONS** | **TOTAL POWER****/****FAN POWER** | **ELECTRIC VOLTAGE /****CABLE CROSS SECTION** | **WATER INLET /****WATER PRESSURE** | **WEIGHT** |
| NEVO-04E | ELECTRIC ONVECTION PATISSERIE OVEN | 750X795X560 | 7 kW/2X0,3 = 0,6 kW | 380-400 VAC 3N 50 Hz220-230 VAC 1N 50 Hz/5X2,5 mm23X6 mm2 | R 3/4/1,5-4 bar | 70 kg net |
| 770X820X610Package dimension | 80 kg Gross weight |



|  |  |
| --- | --- |
| **HEADQUARTER** | **FACTORY** |
| Plevne Caddesi No.40/C | Taşpınar Mevkii No.154 |
| Gülveren-Mamak/ANKARA | Çubuk/ANKARA |
| Tel . | +90 312 363 94 93 | Tel . |  +90 312 837 76 72 |
| Fax. | +90 312 363 94 92 | Fax. | +90 312 837 73 38 |
| [**www.mutasgroup.com**](http://www.mutasgroup.com/) **/** **info@vitalmutfak.com** |