

USAGE AND MAINTENANCE MANUAL

ELE

**ELECTRIC RANGES WITH OVEN**

* **EKF7020**
* **EKF7030**
* **EKF7020K**
* **EKF7030K**
* **EKF9020K**
* **EKF9030K**



# PRESENTATION

# DEAR CUSTOMERS,

* To get the best yield of our products that are in compliance with the International Standards, we highly recommend you to read the user’s manual and have it read to your users for long and continuous usages.
* This manual contains important informations about the secure installation, usage and maintenance of the product and necessary remarks to make the most efficient usage of your device.
* Keep this manual in an easily accessible and safe place to use when necessary.
* Our product is designed for heating and cooking food commodities. Any chemical or liquid substances or similar that can be in contact with the foodstuff, cannot be used for any heat treating that can cause damages for the health.
* The manufacturer cannot be held responsible for any damages from incorrect usage of the device, to people, the environment, or other materials resulting from translation or printing of this booklet.

# INDEX

[PRESENTATION 2](#_Toc515697638)

[INDEX 3](#_Toc515697639)

[SAFETY DETAILS 4](#_Toc515697640)

[TECHNICAL SPECIFICATIONS 5](#_Toc515697641)

[TRANSPORTATION, PLACEMENT AND READY TO INSTALL 7](#_Toc515697642)

[ELECTRICAL CONNECTION 8](#_Toc515697643)

[USAGE 9](#_Toc515697644)

[1-) Switching On 9](#_Toc515697645)

[1.1-) Upper Section 9](#_Toc515697646)

[1.2-) Oven Section 10](#_Toc515697647)

[2-) Switching Off 10](#_Toc515697648)

[CLEANING 10](#_Toc515697649)

[MAINTENANCE AND MALFUNCTION 11](#_Toc515697650)

[Problems and Solutions 11](#_Toc515697651)

[WARRANTY CONDITIONS 12](#_Toc515697652)

[Out of Warranty Cases 13](#_Toc515697653)

[AUTHORIZED SERVICE START-UP PAGE 14](#_Toc515697654)

[Start Up Page 14](#_Toc515697655)

# SAFETY DETAILS

* Do not expose the device to direct sunlight.
* Any kind of flammable or ignitiable solid or liquid such as alchocol and derivaritves, petro-chemical products, wood-plastic materials, curtains, clothes, etc. should not be kept in the area of the device.
* Do not clean the device with high pressured water.
* This device must be installed in accordance with the current regulations and should only be used in a well-ventilated area.
* The instructions should be analysed before the installation and the usage of the device.
* The device is designed for professional usage and should only be used by trained personnel.
* It should not be interfered without the presence of the manufacturer or the authorized service.
* The device or its components cannot be used for any other purpose.
* Apart from the heating and the cooking of the food, it cannot be used as a heater for any purpose.
* The device cannot be left uncontrolled as long as it is on.
* Food compatible gloves must be used to protect hands from the overheating.
* In case of fire or flame in the area where the device is, switch off the safety net which is located in the main circuit connection and then use the fire extinguisher. Water should absolutely not be used, otherwise the flame will sprawl faster.
* The installation and the maintenance should be carried out by the qualified staff autorized by the manufacturer. Serious danger for the user can be arise due to incorrect installations, maintenances or repairs, and the manufacturer cannot be held responsible.

# Technıcal specıfıcatıons

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PRODUCT CODE** | **EKF7020** | **EKF7030** | **EKF7020K** | **EKF7030K** | **EKF9020K** | **EKF9030K** |
| **DIMENSIONS****(mm)** | **A** | **WIDTH**  | 800 | 1200 | 800 | 1200 | 800 | 1200 |
| **B** | **DEPTH** | 730 | 730 | 730 | 730 | 900 | 900 |
| **C** | **HEIGHT** | 850 | 850 | 850 | 850 | 850 | 850 |
| **ELECTRIC POWER** | 15,4 kW | 20,6 kW | 15,4 kW | 20,6 kW | 21 kW | 29 kW |
| **ELECTRIC INLET** | 380-400 VAC 3N PE 50 HZ |
| **CABLE CROSS SECTION** | 5\*4 mm2 | 5\*6 mm2 | 5\*4 mm2 | 5\*6 mm2 | 5\*6 mm2 | 5\*6 mm2 |
| **WEIGHT** | 80 Kg | 140 Kg | 82 Kg | 144 Kg | 95 Kg | 165 Kg |

(A)

(A)



EKF7030, EKF7030K, EKF9030K

EKF7020, EKF7020K, EKF9020K



EKF7020

EKF7020K







EKF7030

EKF7030K





EKF9030K

EKF9020K



(C)

(C)

EKF9020K, EKF9030K

EKF7020, EKF7020K

EKF7030, EKF7030K

# TRANSPORTATION, PLACEMENT AND READY TO INSTALL

* Do not tilt the device during the transportation, carry it upright.
* Use a suitable vehicle to avoid any kind of damages.
* Do not push or drag the device to bear.
* When transporting by pallet jack or forklift, make sure to not damage the device.
* Carry the device with its packaging until the installation area.
* It should be placed under a ventilation system to avoid any kind of bad smell that may occur during cooking process.
* It is recommended to place a suitable sized hood for the ventilation over the device without blocking the outlet of the chimney.
* In case the device is installed next to a wall, a partition, a kitchen furniture etc., make sure they are made by non flammable material or with a suitable thermal insulation coating with a margin of 10 cm, otherwise with a margin of 30 cm.
* Never place a combustible material on top of the device.
* Make a general cleaning before the first usage. You may use soapy water.
* The operating environment and the ventilation system of the device must be between 10°C to 40°C and have a maximum humidity level of %80.
* The device must be installed in accordance within the instructions.
* The protective film on the surface of the device must be stripped off carefully.
* Convenient electrical connection with the required technical specifications must be installed in the area of the device.

# ELECTRICAL CONNECTION

* Technical specification section should be analysed for the appropriate cable to be used for the electrical connection of the device.
* The electrical supply circuit must be done by the authorized staff. Before installation, make sure that your fitment meets the requirements. The device should absolutely not be used without grounding.
* The electrical voltage must be stable for the proper fonction of the device. If the malfunction is caused by the voltage, the replacement of these parts are considered “out of warranty”. Fault detection is based on the service declaration.
* To prevent the device from any short circuit and overcurrent, the device must be supplied with the appropriate fuse control.

****



EKF7020 EKF7030 EKF7020K EKF7030K

EKF9020K EKF9030K

**EQ=GROUNDING SCREW**

**EI=ELECTRICAL CONNECTION**

# usage

* The device is designed for professional usage and should only be used by trained personnel.
* If the device is operated as ungear for a while, it will remove the smoke caused by the protective oils.
* Appropriate cooking pots should be placed on the device.

***B***

***B***

***A***

***E***

***C***

***A***

***D***

***E***

***D***

***C***

Image -1 CONTROL PANNEL

|  |  |
| --- | --- |
| A | Commutator switch |
| B | Thermostat knob |
| C | Commutator lamp |
| D | Section Indicator |
| E | Thermostat Lamp |

## 1-) Switchin On

## 1.1-) Upper Section

* To power the device, turn on the fuse to which the device is connected.
* Set the commutator switch to de requested level. The commutatorlamp will be lit and the plates will star to heat up.

## 1.2-) Oven Section

* Set the thermostat knob to the requested degree. The thermostat lamp will lit and the oven chamber will star to heat.
* When the oven reaches the requested temperature, the lamp will turn off and the heating process will stop.

## 2-) Switching Off

* For the upper section, set the commutator switch to the “0” position. The commutator lamp will turn off and the heating of the plates will end heating.
* For the oven section, set the thermostat button to the “0” position. The lamp will turn off and the heating process will end.

# cleanıng

* Disconnect the wiring of the device before starting the cleaning process.
* When cleaning the device, make sure to prevent water from entering the electrical parts.
* Do not wash the device with high pressure water.
* After each usage, clean the device with a cloth dipped in warm soapy water.
* Do not use abrasive detergent or wire brushes when cleaning the device’s surface.
* Clean completely the device on specific periods with convenient cleaning materials.

# maıntenance and malfunctıon

* The maintenance and the malfunction of the device must be carried out by the authorized service or by a personnel assigned by the manufacturer.
* All connections and repairs must be carried out by the authorized service centers, otherwise, your device will be out of warranty.

|  |  |
| --- | --- |
| Plates do not heat. | 1. Check the fuse to which the device is connected.
2. Check the commutator switch position.
3. If the plates do not heat up after these steps, please contact the **AUTHORIZED SERVICE.**
 |
| The plates do not reach the required temperature.  | 1. Check the commutator switch of the device. If its at low heat, raise it. If the problem persists after increasing the level, please contact the **AUTHORIZED SERVICE.**
 |
| The oven does not heat. | 1. Make sure that the thermostat knob is on de required level of degrees. If it is and the oven does not heat, please contact your **AUTHORIZED SERVICE**.
 |

## Problems and Solutions

# WARRANTY CONDITIONS

* According to the consumer rights law and commercial law of the Ministry of Industry, except in a special case of agreement, sold industrial products by our company has one (1) year of warranty and that period starts from the delivery date of the product.
* The warranty includes all the components of the device against fabrication or faulty workmanship, eliminations of the problems or malfunctions of the device caused by the workmanship and installation errors, replacement of non-repairable parts or the mending of repaired parts that can be reused. It also includes repairings or changes of the components by the authorized personnel, or the labor fee due to the problem under the warranty.
* In order for the warranty conditions to be valid, the maintenance of the components fixed to the device, the maintenance of the product, as indicated in the user’s manual, should be done yearly and montly and the information form must be held after the maintenance to be presented when required.
* The document of the replacement of the component has to be presented for parts warranty claims.
* In order to continue the warranty period, the paid periodic maintenance has to be done by the authorized service and the information form must be held to be presented when required.
* In case of any malfunctions under the warranty period, the time spent in the repairment of the device is added to the warranty period. The repair can be maximum 30 (thirty) days. This period starts when the device is on the service station. In case of the absence of this station, the period will start when the manufacturer or the importer is notified by the product seller.
* In accordance with the regulations of the warranty document implementation fundamentals published by the Ministry of Industry, the warranty deed of the industrial products are the purchase invoices.
* If there is any kind of malfunctions due to both the materail and the workmanship, or assembly faults under the warranty period, the necessary replacement and reparing will be done by our authorized personnel without any charge.

## Out of Warranty Cases

* If the product is used above its intended purpose, standards or capacity specified by the manufacturer,
* In case of the bad locationing of the product, continuous usage and unhealthy environment (ex: required ventilation), not suitable floor or flat platform, lack of convenient gas pressure,
* If the product hasn’t been used as explained in the instruction manual,
* If the fault is caused by inconvenient, worng or careless usage,
* If the malfunction is caused by fluactions in the mains power, a stoke or a meteor lightening, a fire, a flood, an earthquake or similar cases,
* If the special tools and equipments installed or the maintenance and repair are made by any other person than the authorized person,
* When requesting a service, if the installation-start documents or purchase invoices of the product are not presented,
* If the informations on the documents of the installation, start or maintenance has been destroyed or changed,
* If the paid annual or the contractual periodic maintenance of the product has not been done on time by the authorized personnel,
* If unoriginal spare parts have been used,
* Notifications to our authorized services under the warranty period about the malfunctions that could not have been repaired, will make the time-out of the warranty stop only for that specific malfunction. In this case, the authorized service will inform about the compensation or the non-troubleshooting and the expanded warranty period will end in 3 months in any cases,
* Damages caused by the unnecessary loss of time, the maleficience, the revenue loss, or the conduction of the product from the defective location to another,
* Malfunctions of the product due to squalidity are not covered by the warranty,
* The methods to be followed about the fault detection and elimination are determied completely by MUTAŞ’s technical service management and the service matter is taken as basis for the determination of the malfunction.

# AUTHORIZED SERVICE START-UP PAGE

## Start Up Page

* The model and serial number of your device are shown on the “Technical Data” label affixed to the device.
* Select the technical data according to the device model on the nameplate.

**MUST BE FILLED BY AUTHORIZED SERVICE!**

|  |  |
| --- | --- |
| **COMPANY INFORMATIONS** | : |
| **PRODUCT** | : |
| **MODEL** | : |
| **SERIAL NUMBER** | : |
| **PRODUCTION DATE** | : |
| **SERVICE STAMP AND SIGNATURE** | : |
| **PERSONNEL OF THE SERVICE** | : |
| **CONTACT** |  |
| **TEL** | : **0312 837 76 72** |
| **FAX** | : **0312 837 73 38** |
| **E-MAIL** | : **teknikservis@vitalmutfak.com** |

**CONTACT**

|  |
| --- |
| **MUTAŞ MUTFAK ISITMA SİSTEMLERİ SAN. PAZ. İNŞ. TUR. İÇ VE DIŞ TİC.LTD.ŞTİ****HEADQUARTER****ADRES: Plevne Cad. No:40 Gülveren / ANKARA****TEL: (0312) 363 99 33 FAX: (0312) 363 94 92****Web:** [**www.vitalmutfak.com**](file:///C%3A%5CUsers%5Chasan%5CDesktop%5Cwww.vitalmutfak.com) **E-Mail:****info@vitalmutfak.com** |
| **MUTAŞ MUTFAK ISITMA SİSTEMLERİ SAN. PAZ. İNŞ. TUR. İÇ VE DIŞ TİC.LTD.ŞTİ****FACTORY****ADRES: Taşpınar Mahallesi Küme Evleri No:154/A Çubuk / ANKARA****TEL: (0312) 837 76 72 FAX: (0312) 837 73 38****Web:** [**www.vitalmutfak.com**](file:///C%3A%5CUsers%5Chasan%5CDesktop%5Cwww.vitalmutfak.com)**E-Mail:****teknikservis@vitalmutfak.com** |



**AFTER SALES SERVICE**

**For the nearest MUTAŞ/VİTAL Athorized Service, please contact the numbers above.**

**teknikservis@vitalmutfak.com**